    function globalPause(address[] memory _addresses) external returns (address[] memory _updatedAddresses) {
        require(msg.sender == CIRCUIT_BREAKER_ADDRESS, "Circuit Breaker only");
        address _pairAddress;
        uint256 _lengthOfArray = _addresses.length;
+       _updatedAddresses = new address[](_lengthOfArray);
        for (uint256 i = 0; i < _lengthOfArray; ) {
            _pairAddress = _addresses[i];
            try IFraxlendPair(_pairAddress).pause() {
                _updatedAddresses[i] = _addresses[i];
            } catch {}
            unchecked {
                i = i + 1;
            }
        }
    }
